Parth Mehrotra

Hari Raval - Nimai’s Bliss Kitchen.

This package should contain

* 3x Slide Show SD-Cards
* 1x Order View SD-Cards

Definitive Reference, and some things that could go wrong.

To start a slide show.

1. Connect the Raspberry Pi to a TV, and a Keyboard (Temporarily)
2. Insert SD-Card for the Slide Show program
3. Connect the Raspberry Pi to power.
4. You should first see a colorful image, then text. Allow the text to keep outputting util you see a prompt for username
   1. USERNAME: pi
   2. PASSWORD: raspberry
5. After pressing return after entering your password, the pi should boot into a graphical screen that has a black box in the center with some instructions.
6. By typing the word run and pressing return, the slideshow will start displaying the images located in the folder called slides. This folder is located on the desktop.

To Change the Images in the slideshow program

1. Reach Step 5 above, but do not start the slideshow.
2. Insert a flash drive.
3. A prompt will ask what you want to do with the flash drive you’ve just inserted
4. Continue with the default, it should open the flash drive in a file explorer.
5. Double click on the slides folder on the desktop
6. Name the images in the following format
   1. 0.jpg, 1.jpg,...,n.jpg
7. Once you’re satisfied with images, and their order, type run in the black box titled LXTerminal

To launch the OrderViewer

1. Connect the Raspberry Pi to a TV, **WiFi dongle**, and a Keyboard (Temporarily)
2. Insert SD-Card for the Slide Show program
3. Connect the Raspberry Pi to power.
4. You should first see a colorful image, then text. Allow the text to keep outputting util you see a prompt for username
   1. USERNAME: pi
   2. PASSWORD: raspberry
5. You should boot into a green desktop. If you have not already configured the internet, Double Click “WiFi Config” on the desktop.
   1. If “Adapter” is empty, and you can’t select wlan0, stop.
      1. is the WiFi dongle connected?
      2. is it lighting up?
      3. reboot
   2. Click Scan
   3. Click Scan in the Scan Results window
   4. Double Click your network
   5. Enter your password in the “PSK” field.
   6. Click “Add”
   7. This will configure your wifi. You will not have to repeat this step in the future.
6. Open Epiphany to ensure the internet is working
7. Then click on the orderviewer.html.
   1. This should open in epiphany, if it doesn’t right click on it and press open with… and select epiphany.
8. You can press F11 to enter full screen
9. Your pending orders will be displayed here. When you complete an order, simply tap on it, it will go away, and it’s “status” will not be pending anymore. The orders stay in parse (just incase something goes wrong).